Olimp double curtain rod, 19/19 mm, 150 cm,  Cylinder Ball, antique

PRODUCT FEATURES:
• The auction concerns a ready-to-install double metal curtain rod with full equipment
• Color: antique
• Length: 150cm
• End: Cylinder Ball
• All elements of the set are galvanized, making them resistant to abrasion, rust and discoloration
• A hard metal alloy tube with increased wall thickness is resistant to bending
• The colors of the metal are subdued, they do not stand out strongly in the background, making the curtain rod fit into any interior
• The wheels on the inside are covered with a plastic coating, thanks to which they move silently along the tube
• Universal installation: on the ceiling or wall

 SET ELEMENTS:
• Metal tube with a diameter of 19 mm - 2 pieces. Curtain rods up to 250 cm long are delivered as a whole, and above 250 cm in two equal parts
• Double wall brackets - (2 pcs. up to 250 cm, 3 pcs. above 250 cm)
• Quiet circles with a clip - 1 piece for every 10 cm of the length of each tube
• Decorative endings - 2 pieces to choose from
• Luna endings - 2 pcs. (for the rear tube)
• Set of mounting screws and dowels - 3 pcs. for each bracket
• Pipe connector (only for curtain rods over 250 cm)

TYPE OF UPDOOR:
A quiet circle with a clip
The distance between the upper part of the clip and the tube is 1.6 cm

MEASUREMENT METHOD:
[image: ]

Window recess width + approx. 40 cm
In order to select the appropriate length of the curtain rod tube, it is recommended that it be at least 40 cm wider than the window recess (20 cm on each side).
The length given in this auction refers to the length of the tube itself.
Assembly method:
Attention! 
Do not install brackets on the ends of the pipe to prevent it from bending. A properly installed bracket is at least 10 cm from the edge of the pipe.
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