Triple ceiling curtain rod with PVC safety pin, 150 cm, white

PRODUCT FEATURES:
• The auction concerns a complete PVC ceiling curtain rod with full accessories, 150 cm long
• The attractive price is the result of independent production of all elements on our machines
• Curtain rod made of high-quality raw material from a German company, ensuring durability for years
• The rail design is simple, classic, proven by thousands of customers, which guarantees lightness and easy and stable installation
• The width of the rail and the arrangement of the tracks prevents the curtains from overlapping, ensuring smooth movement of the curtains
• Product dedicated to modern interiors with built-in ceilings, hotels and traditional rooms

SET ELEMENTS:
• 3-track white rail, 150 cm long
• Fastening: safety pin with roller
• End plug: 2 pcs
• A set of dowels with screws in the appropriate number depending on the length of the curtain rod
• Plugs for mounting holes (for screws)

TYPE OF UPDOOR:

Safety pin with roller
Recommended for heavy curtains. The curtain/curtain with safety pins can be pulled out from the curtain rod and put into the wash, which saves time.
Quantity: 45 pcs.

MEASUREMENT AND INSTALLATION METHOD:

Window recess width + approx. 40 cm
In order to select the appropriate rail length, it is recommended that it be at least 40 cm wider than the window recess (20 cm on each side).
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