PVC ceiling rail curtain rod complete with clip, 1st track, 150cm, black

PRODUCT FEATURES:
· The auction concerns a complete PVC ceiling curtain rod with full accessories, 150 cm long
· The attractive price is the result of independent production of all elements on our machines
· The curtain rod is made of high-quality raw material from a German company, ensuring durability for years
· The rail design is simple, classic, proven by thousands of customers, which guarantees lightness and easy and stable installation.
· The width of the rail and the arrangement of the track prevents the curtains from overlapping, ensuring smooth sliding of the curtains
· The product is dedicated to modern interiors with built-in ceilings, hotels and traditional rooms

SET ELEMENTS:
· 1-track black rail, 150 cm long
· Updo: clip with a roll
· End plug - 2 pcs
· A set of dowels with screws in the appropriate quantity 
· Plugs for mounting holes (for screws)

Clip with a roller
Standard fastening used for PVC rails. There are teeth on the inside of the frog that prevent curtains from slipping.
Quantity: 15 pcs.
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MEASUREMENT AND INSTALLATION METHOD:
Window recess width + approx. 40 cm
In order to select the appropriate rail length, it is recommended that it be at least 40 cm wider than the window recess (20 cm on each side).
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