PVC ceiling rail curtain rod complete with a clip, 1st track, 250cm, white

PRODUCT FEATURES:
• The auction concerns a complete PVC ceiling curtain rod with full accessories, 250 cm long
• The attractive price is the result of independent production of all elements on our machines
• Curtain rod made of high-quality raw material from a German company, ensuring durability for years
• The rail design is simple, classic, proven by thousands of customers, which guarantees lightness and easy and stable installation
• The rail width and track arrangement prevents curtains from overlapping, ensuring smooth curtain movement
• Product dedicated to modern interiors with built-in ceilings, hotels and traditional rooms

SET ELEMENTS:
• 1-track white rail, 250 cm long
• Clip updo with a roller
• End plug - 2 pcs
• A set of dowels and screws in the appropriate quantity 
• Plugs for mounting holes (for screws)

Clip with a roller
Standard fastening used for PVC rails. There are teeth on the inside of the frog that prevent curtains from slipping.
Quantity: 25 pcs.
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MEASUREMENT AND INSTALLATION METHOD:
Window recess width + approx. 40 cm
In order to select the appropriate rail length, it is recommended that it be at least 40 cm wider than the window recess (20 cm on each side).
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