**Electric bicycle HIMO A16+, White**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| Manufacturer | HIMO |
| Size of Tyre | 40,6 cm (16") |
| Voltage | 36 V |
| Battery | 7.8 Ah |
| Electric Distance | 35 km |
| Boost Distance | 70 km |
| Power | 350 W |
| Model | A16+ |
| Product colour | White |
| Net Weight | 20 kg |
| Max. Speed | 25 km/h |
| Front brake | Mechanical disc brake |
| Rear brake | Mechanical disc brake |
| Charging time | 6 h |
| Payload | 120 kg |
| Material | Aluminum alloy |
| Foldable | Yes |
| Handgrip material | TPR |
| Brake handle | Left/Right |
| Tire | Rubber pneumatic tire |
| Air pump | No |
| Type of batteries | Removable/Portable charging battery |
| Dimensions (LxWxH) | 1440x530x1080 mm |
| Recommended height | 132 -170 cm |
| Number of gears | 7 |
| Fenders | Yes |

 |